|  |  |  |
| --- | --- | --- |
|  | Buta-Palace Rider Video |  |
|  |  |  |
| **KRAMER VP-8x8A** | **8x8 commutator signals** |  |
| **KRAMER VP-727T** | **Remote Control Panel In-CTRL (control)** | **2** |
| **KRAMER VP-727** | **8-input switcher / scaler functions dimming and special effects when switching (switcher)** | **2** |
| **ScreenMaxx 20** | **Automatic screen MW ScreenMaxx 20 400x400 cm (390h293 cm) (white square)** | **4** |
| **LC-XT5** | **Multimedia Projector LCD, Resolution XGA (1024x768 pixels, up to 1280 \* 1024 pixels with compression), the brightness of 15,000 ANSI Im, ZOOM, optical keystone correction, vertical and horizontal contrast 2000 \* 1, weight 43 kg, the ability to work in a vertical position, without lens chetyrehlampovy light unit** | **4** |